{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Materialer","Mængdeliste","Bestilligsliste"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Materialer","index":0,"n_rows":41,"n_cols":24,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["Hovedmenu",null,"valg 1","valg 1.1",null,"valg 2","valg 2.1",null,"valg 3","valg 3.1",null,"valg 4 ","valg 4.1",null,"valg 5","valg 5.1",null,"valg 6","valg 6.1",null,"valg 7","valg 7.1",null,"valg 8"]
[]
["Kategori",null,"Træ","Bræddelængde",null,"Plader","Plademål",null,"Gips","Plademål_gips",null,"Stål","Stålmål",null,"Isolering","Isolering_Dim",null,"Skruer","Skrue_Dim",null,"Beslag","Beslag_Dim",null,"Murergrej"]
["Træ",null,"Stolpe",1800,null,"Plader","900x1200",null,"Gipsplade 13 mm. GDS/hobby","900x1200",null,"Bundstål",2500,null,"Rockwool","600x900",null,"Spånskrue","5x100",null,"vinkel uden ribbe","90x90x2"]
["Plader",null,"Stolpe 75x75 mm. Uhøvlet",2100,null,"Krydsfiner","900x2400",null,"Gipsplade 13 mm. MK-Godkendt","900x2400",null,"Top/bundstål 45mm.",null,null,"Knauf",null,null,"Beslag skrue",null,null,"Vinkel med ribbe"]
["Gips",null,"Stolpe 97x97 mm. Uhøvlet",2400,null,"Krydsfiner 4 mm.  Uden fer/not","900x2500",null,"Gipsplade 15 mm. Brandgips","900x2500",null,"Top/bundstål 70mm.",null,null,"Glasuld",null,null,"Karmskrue"]
["Stål",null,"Stolpe 125x125 mm. Uhøvlet",2700,null,"Krydsfiner 6 mm.  Uden fer/not","900x2700",null,"Gipsplade 13 mm. Skolegips","900x2700",null,"Top/bundstål 95mm.",null,null,"Papiruld"]
["Isolering",null,"Stolpe 75x75 mm. Høvlet",3000,null,"Krydsfiner 9 mm.  Uden fer/not","900x3000",null,"Fibergips","900x3000",null,"Top/bundstål 120mm."]
["Skrue",null,"Stolpe 90x90 mm. Høvlet",3300,null,"Krydsfiner 12 mm. Uden fer/not","1200x2400",null,"Fibergips 12mm. Med spartelkant","1200x2400",null,"Top/bundstål 145mm."]
["Beslag",null,"Reglar 45x45 mm.  Trykimprægneret Høvlet",3600,null,"Krydsfiner 15 mm. Uden fer/not","610x2440",null,"Fibergips 15mm. Med spartelkant",null,null,"Stålregler"]
["Murergrej",null,"Reglar 45x95 mm.  Trykimprægneret Høvlet",3900,null,"Krydsfiner 18 mm. Uden fer/not","1220x2440",null,"Fibergips 12mm. Uden spartelkant",null,null,"Stålregel 45 mm. C profil"]
[null,null,"Relar 45x45 mm.  Ubehandlet, Høvlet",4200,null,"Krydsfiner 21 mm. Uden fer/not","1250x2500",null,"Fibergips 15mm. Uden spartelkant",null,null,"Stålregel 70 mm. C profil"]
[null,null,"Relar 45x95 mm.  Ubehandlet, Høvlet",4500,null,"Krydsfiner 12 mm. Med fer/not (gulv/tag)",null,null,null,null,null,"Stålregel 95 mm. C profil"]
[null,null,"Konstruktionstræ 45x120 mm. Ubehandlet",4800,null,"Krydsfiner 15 mm. Med fer/not (gulv/tag)",null,null,null,null,null,"Stålregel 120 mm. C profil"]
[null,null,"Konstruktionstræ 45x145 mm. Ubehandlet",5100,null,"Krydsfiner 18 mm. Med fer/not (gulv/tag)",null,null,null,null,null,"Stålregel 145 mm. C profil"]
[null,null,"Konstruktionstræ 45x195 mm.Ubehandlet",5400,null,"Krydsfiner 21 mm. Med fer/not (gulv/tag)",null,null,null,null,null,"Stålregel 70 mm. Lydprofil"]
[null,null,"Konstruktionstræ 45x245 mm. Ubehandlet",5700,null,"Støbfiner",null,null,null,null,null,"Stålregel 95 mm. Lydprofil"]
[null,null,"Konstruktionstræ 45x295 mm. Ubehandlet",6000,null,"Støbfiner 12 mm.",null,null,null,null,null,"Stålregel 120 mm. Lydprofil"]
[null,null,"Konstruktionstræ 45x120 mm.  Trykimprægneret",6300,null,"Støbfiner 15 mm.",null,null,null,null,null,"Stålregel 160 mm. Lydprofil"]
[null,null,"Konstruktionstræ 45x145 mm.  Trykimprægneret ",6600,null,"Støbfiner 18 mm."]
[null,null,"Konstruktionstræ 45x195 mm.  Trykimprægneret ",6900,null,"Støbfiner 21 mm."]
[null,null,"Lægter 38x57mm. Ubehandlet",7200,null,"OSB"]
[null,null,"Lægter38x73 mm.  Ubehandlet",7500,null,"OSB 12 mm. Uden fer/not"]
[null,null,"Lægter 38x57mm. Trykimprægneret",7800,null,"OSB 15 mm. Uden fer/not"]
[null,null,"Lægter38x73 mm.  Trykimprægneret",8100,null,"OSB 18 mm. Uden fer/not"]
[null,null,"Forkalningsbræt 19x100 mm. Uhøvlet",null,null,"OSB 21 mm. Uden fer/not"]
[null,null,"Forkalningsbræt 25x100 mm. Uhøvlet",null,null,"OSB 12 mm. Med fer/not (gulv/tag)"]
[null,null,"Forkalningsbræt 22x100 mm. høvlet",null,null,"OSB 15 mm. Med fer/not (gulv/tag)"]
[null,null,"Trykimprægneret brædder 16x100 mm.",null,null,"OSB 18 mm. Med fer/not (gulv/tag)"]
[null,null,"Trykimprægneret brædder 19x75 mm.",null,null,"OSB 21 mm. Med fer/not (gulv/tag)"]
[null,null,"Trykimprægneret brædder 19x100 mm."]
[null,null,"Trykimprægneret brædder 19x125 mm."]
[null,null,"Trykimprægneret brædder 25x100 mm."]
[null,null,"Trykimprægneret brædder 25x125 mm."]
[null,null,"Trykimprægneret brædder 25x150 mm."]
[null,null,"Trykimprægneret brædder 25x175 mm."]
[null,null,"Trykimprægneret brædder 19x200 mm."]
[null,null,"Terrassebrædder 21x95 mm.  Trykimprægneret"]
[null,null,"Terrassebrædder 28x120 mm.  Trykimprægneret"]
[null,null,"Terrassebrædder 28x145 mm.  Trykimprægneret"]
[null,null,"Terrassebrædder lærk"]

{"sheet":"Mængdeliste","index":1,"n_rows":5,"n_cols":8,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[null,"Bemærk at kolonne C er skjult.",null,null,null,null,null,"Filen skal gemmes som xlsm"]
[]
[]
["Tiltænkt","Kategori","Dimension","Produkt","Dimension","Stk.","Pris pr. stk","I alt"]
[null,null,{"$f":"INDEX(Materialer!C3:X3,MATCH(B5,Materialer!C3:X3,0)+1)","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"IF(F5,F5*G5,\"\")","v":""}]

{"sheet":"Bestilligsliste","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}