{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Ark1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":18,"n_cols":24,"rows_kept":18,"cut":false,"hidden":false,"merged":[[11,7,12,10],[0,3,1,15],[7,4,8,7],[7,9,8,11],[4,18,4,20],[3,3,3,5],[4,3,4,5],[3,8,3,10],[4,8,4,10],[3,13,3,15],[4,13,4,15]]}
[null,null,null,"Indtast værdi"]
[]
[]
[null,null,null,"Varmepumpe måler",null,null,null,null,"Prodceret Kwh varme",null,null,null,null,"Prodceret varm vand"]
[null,null,null,40,null,null,"Kwh",null,100,null,null,"Kwh",null,8,null,null,"m3"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vand ind",10,"grader"]
[null,null,null,null,"SCOP VÆRDI",null,null,null,null,{"$f":"(N5*Q11)+I5/D5","v":390.41999999999996},null,null,null,null,null,null,"Vand ud",47.3,"grader"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Leveret",{"$f":"R8-R7","v":37.299999999999997},"grader"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"R9*X15","v":48.489999999999995},"Kwh. Pr. m3"]
[null,null,null,null,null,null,null,"Gem data"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Der skal bruges 1,3 kWh for at opvarme 1 kbm vand 1 grad. Så hvis vandet skal varmes fra fx 10 grader til 50 grader skal der bruges 40 x 1,3 = 52 kWh til opvarmning pr kbm."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.3]
[]
[]
["Dato","VP","Prod.Kwh","Prod.vand","Scop"]