{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["1212"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1212","index":0,"n_rows":8,"n_cols":2,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,1],[5,0,5,1]]}
["Beregning af nye kordinat, \ndrejer mod uret omkring punktet X=0,Y=0"]
["Indtast"]
["X",-97.539000000000001]
["Y",-59.347000000000001]
["Grader",90]
["Resultet"]
["X ny",59.346999999999994]
["Y ny",-97.539000000000001]