{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Ark1","Calculations"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":102,"n_cols":11,"rows_kept":102,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Part number:",{"$f":"(B8*D8*10000)+(B9*D9*10000)+(B10*D10*10000)+B12*D12+B13*D13+B14*D14+B15*D15+B16*D16+B17*D17+B18*D18+B19*D19+B20*D20+B21*D21","v":350200},{"$f":"IF(B24=FALSE,D23,D24)","v":"-"},{"$f":"10000*(B26*(D26*B8+E26*B9+F26*B10)+B27*(D27*B8+E27*B9+F27*B10)+B28*(D28*B8+E28*B9+F28*B10)+B29*(D29*B8+E29*B9+F29*B10)+B30*(D30*B8+E30*B9+F30*B10)+B31*(D31*B8+E31*B9+F31*B10)+B32*(D32*B8+E32*B9)+B33*(D33*B8+E33*B9))+(((B35*D35)+(B36*D36)+(B37*D37)+(B38*D38)+(B39*D39)+(B40*D40)+(B41*D41)+(B42*D42))*1000)+(((B44*D44)+(B45*D45)+(B46*D46)+(B47*D47)+(B48*D48)+(B49*D49)+(B50*D50)+(B51*D51)+(B52*D52))*100)+((B54*10)+(B55*20)+(B56*30)+(B57*40)+(B58*50)+(B59*60)+(B60*70)+(B61*80)+(B62*90))+(B64*D64+B65*D65+B66*D66+B67*D67+B68*D68+B69*D69)","v":143210},null,{"$f":"IF(B72=FALSE,D71,D72)","v":"-"},{"$f":"((B74*D74+B75*D75+B76*D76+B77*D77+B78*D78+B79*D79+B80*D80+B81*D81+B82*D82)*100000)+((B84*D84+B85*D85+B86*D86+B87*D87+B88*D88+B89*D89+B90*D90)*10000)+((B92*D92+B93*D93+B94*D94+B95*D95+B96*D96+B97*D97)*1000)+((B99*D99+B100*D100+B101*D101+B102*D102)*100)","v":49000},null,null,{"$f":"C2&D2&E2&G2&H2","v":"350200-143210-49000"}]
[null,null,null,null,null,null,null,12345]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(C2,1)=\"0\",\"0\"&C2,C2)&D2&IF(LEN(E2)=5,\"0\"&E2,E2)&G2&IF(LEN(H2)=5,\"0\"&H2,H2)","v":"350200-143210-049000"}]
[null,{"$f":"IF(B75+B101=1,\"HE std. st./std. st. pison ring must be comb.\",\"\")","v":""}]
[null,null,"Options","Parameters",null,null,null,null,null,null,{"$f":"TEXT(H3,REPT(\"0\",6))","v":"012345"}]
[null,"Product Series"]
[null,true,"str35",35]
[null,false,"str50",50,null,null,null,"Noget af det ser rigtig godt ud Hans."]
[null,false,"str60",60,null,null,null,"Men dog sætter den konsekvens nul foran med din formel, så når jeg ændrer f.eks B26 til falsk og B27 til sand, så får jeg 0143210 i stedet for kun 143210 ( 6 cifre )"]
[null,"Stroke Length",null,null,null,null,null,"Kan dog ikke gennemskue at lave en for hver situation, selvom det nok er løsningen."]
[null,false,"50",50,null,null,null,"Evt. en betingetformatering måske ville kunne."]
[null,false,"100",100]
[null,false,"150",150]
[null,true,"200",200]
[null,false,"250",250]
[null,false,"300",300]
[null,false,"350",350]
[null,false,"400",400]
[null,false,"500",500]
[null,false,"750",750]
[null,"Low Noise"]
[null,true,"Standard","-"]
[null,false,"Low Noise","+"]
[null,"Gearing"]
[null,false,"05/04 (24VDC only)",5,4]
[null,true,"14/14/19",14,14,19]
[null,false,"19/17/43",19,17,43]
[null,false,"27/24/66",27,24,66]
[null,false,"51/49/81",51,49,81]
[null,false,"71/84/100",71,84,0]
[null,null,"100",0]
[null,null,"139",39]
[null,"Voltage"]
[null,false,"12Vf",1]
[null,null,"12Vf - EN/UL 60.601",2]
[null,true,"24Vf",3]
[null,false,"24V",4]
[null,null,"36Vf",5]
[null,null,"36V",6]
[null,false,"24Vf - EN/UL 60.601",7]
[null,null,"24V - EN/UL 60.601",8]
[null,"Pitch/Nut"]
[null,true,"2mm std. - str35",2]
[null,false,"3mm std. - str50",3]
[null,false,"4mm std. - str60",4]
[null,false,"2mm std. low temp. grease",5]
[null,false,"2mm std. high temp. grease",6]
[null,false,"'Spline' and emer. low.",7]
[null,false,"Nut w/magnets (positioning)",1]
[null,false,"3mm std. low temp. grease",8]
[null,false,"3mm std. high temp. grease",9]
[null,"Cable Length"]
[null,true,"1 meter",1]
[null,false,"2 meters",2]
[null,false,"3 meters",3]
[null,false,"4 meters",4]
[null,false,"5 meters",5]
[null,false,"6 meters",6]
[null,false,"7 meters",7]
[null,false,"8 meters",8]
[null,false,"9 meters",9]
[null,"Cable & Connector"]
[null,true,"Black, no connector",0]
[null,null,"Grey, no connector",1]
[null,false,"Black, Molex",2]
[null,null,"Grey, Molex",3]
[null,null,"Black, DIN",4]
[null,null,"Grey, DIN",5]
[null,"Puls Sensors"]
[null,true,"Without puls sensors","-"]
[null,false,"With puls sensors","+"]
[null,"Steel & IP Class"]
[null,true,"Std. steel, IP66",0]
[null,false,"Std. steel, IP69",9]
[null,false,"AISI304, IP66",1]
[null,false,"AISI316, IP66",2]
[null,false,"AISI304, IP69",3]
[null,false,"AISI316, IP69",4]
[null,false,"AISI316, IP69K",6]
[null,false,"AISI304, IP68, ATEX",7]
[null,false,"AISI316, IP69., ATEX",8]
[null,"Brackets"]
[null,true,"PA",0]
[null,false,"PA w/clevis",1]
[null,false,"Alu",2]
[null,false,"Alu w/clevis",3]
[null,true,"AISI316",4]
[null,false,"AISI316 w/clevis",5]
[null,false,"Alu w/spherical bearings",6]
[null,"Tube Color"]
[null,false,"Black, RAL9005, shine 25",0]
[null,false,"Grey, RAL9006, shine 30",1]
[null,false,"Light Blue, Pantone 2718U",2]
[null,false,"White, RAL9003, shine 70",3]
[null,false,"Grey, RAL7004",4]
[null,true,"AISI",9]
[null,"Piston Ring Color"]
[null,true,"Black",0]
[null,false,"Grey",1]
[null,false,"Black IP69 std. steel",2]
[null,false,"AISI IP69",9]

{"sheet":"Calculations","index":1,"n_rows":10,"n_cols":11,"rows_kept":10,"cut":false,"hidden":true,"merged":[[2,1,2,3],[2,5,2,7],[2,9,2,11]]}
["Calculations - please do not touch!!!"]
[]
[null,"Schedule a",null,null,null,"Schedule b",null,null,null,"Schedule c"]
[null,"Qty. (<)","Trans. Price","TP60",null,null,"Trans. Price",null,null,null,"Trans. Price"]
[null,3,0.7,0.7,null,null,0.8,null,null,null,0.7]
[null,15,0.59040000000000004,0.68,null,null,0.72,null,null,null,0.59040000000000004]
[null,30,0.55500000000000005,0.66,null,null,0.70399999999999996,null,null,null,0.55500000000000005]
[null,70,0.45,0.64,null,null,0.68799999999999994,null,null,null,0.53039999999999998]
[null,150,0.37,0.62,null,null,0.6804,null,null,null,0.52]
[null,500,0.34,0.6,null,null,0.65600000000000003,null,null,null,0.504]